|  |  |
| --- | --- |
| Actually this firmware is working. Because the OS installed the driver for the scanner at ‘USB Mode’, the scanner is still working at USB Mode when configure at ‘USB HID KBW Mode’. So please remove the original driver. Follow the steps below.    [For PC that connected SD380 before]  -Plug the scanner on PC.  -Set the scanner default by scanning: ‘Set All Default’ -> ‘Save Parameters’.  -Un-plug the USB cable and plug again to reboot the scanner. The scanner will be working at ‘USB Mode’.    -On PC, open ‘Device Manager’. Expand ‘Human Interface Devices’.  -Right-Click on each ‘USB Input Device’, select ‘Properties’.  -Click ‘Details’.  -In ‘Property’ dropdown menu, select ‘Hardware IDs’.  -Find ‘VID\_040B & PID\_6543’ which is for SD380.  -Check all the devices one by one. There are 2 devices to be found.  -Right-Click on the 2 found ‘USB Input Devices’. Select ‘Uninstall’ to remove the 2 devices separately.  -Scan: ‘Start Configuration’ -> ‘USB HID Keyboard Mode ON’ -> ‘End Configuration’ -> ‘Save Parameters’.  -Un-plug the USB cable and plug again to reboot the scanner. At this stage, the scanner will be working at ‘USB HID Keyboard Mode’.    [For a PC that first connecting SD380]  We will make ‘USB HID KBW Mode-ON’ as default on SD380 for you. When receive it and connect it on a PC that first connecting SD380, the OS will install corresponding driver automatically. You don’t have to do anything and it will be working on both POS and PC.    The firmware for SD380 will keep at:  S32V7.03.20A0900    2017.09.13 | На самом деле это прошивка работает. Поскольку ОС установила драйвер для сканера в режиме USB, сканер все еще работает в режиме USB при настройке в режиме USB HID KBW. Поэтому, пожалуйста, удалите оригинальный драйвер. Выполните следующие действия:  [Для ПК, подключенного ранее к SD380]  - Запустите сканер на ПК.  - Установите сканер по умолчанию, выполнив сканирование: «Установить все по умолчанию» -> «Сохранить параметры».  - Отключите USB-кабель и снова подключите его снова для перезагрузки сканера. Сканер будет работать в режиме USB.  - На ПК откройте «Диспетчер устройств». Разверните «Устройства интерфейса пользователя».  - Нажмите правой клавишей на каждое «USB-устройство ввода», выберите «Свойства».  - Нажмите «Подробности».  В раскрывающемся меню «Свойство» выберите «Идентификаторы оборудования».  - Find 'VID\_040B & PID\_6543', который предназначен для SD380.  - Проверьте все устройства один за другим. Существует 2 устройства.  КАРТИНКА  Щелкните правой кнопкой мыши на 2 найденных «USB-устройствах ввода». Выберите «Деинсталлировать», чтобы удалить 2 устройства отдельно.  КАРТИНКА  Сканировать: «Начать настройку» -> «USB HID Keyboard Mode ON» -> «End Configuration» -> «Сохранить параметры».  -Отключить USB-кабель и снова подключите его для перезагрузки сканера. На этом этапе сканер будет работать в режиме USB HID Keyboard.  [Для ПК, впервые подключающего SD380]  Мы сделаем режим работы «USB HID KBW Mode-ON» по умолчанию на SD380 для вас. Когда вы получите его и подключите к ПК, который сначала подключит SD380, ОС автоматически установит соответствующий драйвер. Вам не нужно ничего делать, и он будет работать как на POS, так и на ПК.    Прошивка для SD380 будет храниться в:  S32V7.03.20A0900 2017.09.13 |
|  |  |